| ###  | Page Index

How to set-up xtelsio TAPI for snom:
1. Download and Installation
Download und extract xtelsio_TAPI_for_snom_setup.zip. Run setup.exe and follow the dialogs.
2. TAPI Driver Configuration
You can open the driver configuration via: [Start > Programs > xtelsio_TAPI_for_snom > xtelsio TAPI for snom - Configuration > Configure...].
Hint: At first, only one TAPI line is supported Double-clicking the TAPI line opens the dialog shown right. |
Futher hints for configuration see: Connection Actions URL
If these settings are done the TAPI driver should work now.
5. Test with xtelsio CTI Client lite
"xtelsio CTI Client lite" is a freeware TAPI application. Download and extract xtelsio_CTI_Client_lite_setup.zip. Run setup.exe and follow the dialogs. Start xtelsio CTI Client. Select [Options > TAPI-Devices > Add] You should see your snom device in the dialog. Double-clicking on the "snom Line" closes the dialog and inserts the device in the device list. Close this dialog with [OK]. A Location config dialog may appear, if location parameters are unknown. Now you can enter a phone number right to the dial button and dial it by pressing the enter key or by mouse click.