Installation • Configuration Pages: • FAQ
Connection • Dial • Action URLs • Extended settings
Up >> | ### Connection | Page Index

> <h4>Connection Settings
> | TAPI for snom - Line Configuration
> IP Address | = IP address of the phone
> Port | = HTTP port for telephone web configuration; default=80
> Authentication, Username, Password | If you enter the IP address of your phone into web browser, a username and password my be queried. The same credentials are entered here.
> Test | If the test indicates an error, please check the connection parameters in your web browser. Enter the IP address of your phone in web browser.
> Note 1: DECT phones are not supported. Note 2: Please check also whether the correct local IP address of your computer is selected on the tab "Action URLs" or "Local IP".