TAPI for snom Phone
Installation • Configuration Pages: • FAQ
Up >> | ### Installation | Page Index
Test with Outlook or phone.exe

How to set-up xtelsio TAPI for snom:
1. Download and Installation
Download und extract xtelsio_TAPI_for_snom_setup.zip. Run setup.exe and follow the dialogs. You will need Administator rights.
2. TAPI Driver Configuration
You can open the driver configuration via: [Start > Programs > xtelsio_TAPI_for_snom > xtelsio TAPI for snom - Configuration > Configure...].
| xtelsio TAPI for snom - Configuration
| snom Line1
To configure the TAPI line, use the lower button [Settings...]. => <a href="config_dialogs.htm">Configuration Dialogs</a> Hints: The button [Delete] can be used only for the last TAPI Line. The state "closed" means only that the TAPI Line was currently not open by any TAPI application.
2.1. Configure Telephone IP
Configure the Phone IP address in the dialog [<a href="pp_conn.htm">Connection</a>].
2.2. Configure Actions URLs
Configure the Actions URLs in dialog [<a href="pp_actions_url.htm">Aktions URL</a>]. The Actions URLs are needed to detect and display incoming and outgoing calls. Hint: If the Actions URLs do not work, no incoming calls are displayed.
If these settings are done the TAPI driver should work now.
Test with Outlook
3. Hints for Administrators
Terminal Server Installation